

|  |  |
| --- | --- |
| 電　　話 | Tel: 3793 4652 |
| 圖文傳真 | Fax: 2116 0822 |
| 電郵地址 | Email: gesm12@landsd.gov.hk |
| 本署檔號 | Our Ref.: LD SMS/COS/40/9 |
| 來函檔號 | Your Ref. 0111 |

覆函請註明本署檔號

Please quote our reference in response to this letter.

|  |
| --- |
| 我們矢志努力不懈，提供盡善盡美的土地行政服務。 |
| We strive to achieve excellence in land administration. |
| 新界荃灣青山公路382至392號中染大廈29樓2901-03 及 05-06室 |
| 2901-03 & 05-06, 29/F, CDW Building, 382-392 Castle Peak Road, Tsuen Wan, N.T. |
| 網址: Website:www.landsd.gov.hk |

**地　政　總　署**

**Slope Maintenance Section**

LANDS DEPARTMENT

## By Post and Fax (Fax No. 3922 9797)

## 15 April 2021

AECOM Asia Company Limited

12/F Grand Central Plaza, Tower 2

138 Shatin Rural Committee Road

Shatin, Hong Kong

Attn.: Mr. Victon Wong (Project Manager)

Dear Sirs,

##### Agreement No. CE 27/2019 (GE)

##### 2020-2023 Maintenance of Lands Department Slopes

##### in the Southern Regions – Design and Construction

##### Comments on Recurrent MM/EI Records

**Batch No. MMEI0142**

I refer to your above-referenced submission of Recurrent MM/EI records.

The MM/EI records for a feature listed in the attached table have been selected for audit. Our findings are provided in the attached table for your follow-up action. Please take these comments into consideration when finalizing the MM/EI records. Please be reminded to arrange updating of the slope data in SIS of GEO for relevant feature as necessary.

I hereby return the draft MM/EI records submitted under the captioned batch for your necessary action please.

Yours faithfully,

( Kenneth S T KWONG )

for Chief Geotechnical Engineer / Slope Maintenance

file thro’ STO/1 & TO/11

### KSTK/SHWY/kstk

| Agreement No. CE 27/2019 (GE)  Comments on Recurrent MM & EI Reports submitted under Batch No. MMEI0142 | | | |
| --- | --- | --- | --- |
| **Batch No. (MMEI)** | **ID in the Batch** | **Feature No.** | **LandsD’s Comments** | |
| 0142 | 8 | C1142 | (1) O - Based on the information provided, it appears that the wall is less than 3m high. Is it registrable? (2) 1 - 1 | |